|  |  |  |
| --- | --- | --- |
| **NETWORK** | [**Technology**](https://www.gsmarena.com/network-bands.php3) | [GSM / CDMA / HSPA / CDMA2000 / LTE / 5G](https://www.gsmarena.com/oppo_find_x7_ultra-12752.php) |
|  |  |

|  |  |  |
| --- | --- | --- |
| **LAUNCH** | [**Announced**](https://www.gsmarena.com/glossary.php3?term=phone-life-cycle) | 2024, January 08 |
| [**Status**](https://www.gsmarena.com/glossary.php3?term=phone-life-cycle) | Coming soon. Exp. release 2024, January 12 |

|  |  |  |
| --- | --- | --- |
| **BODY** | [**Dimensions**](https://www.gsmarena.com/oppo_find_x7_ultra-12752.php) | 164.3 x 76.2 x 9.5 mm (6.47 x 3.00 x 0.37 in) |
| [**Weight**](https://www.gsmarena.com/oppo_find_x7_ultra-12752.php) | 221 g (7.80 oz) |
| [**Build**](https://www.gsmarena.com/glossary.php3?term=build) | Glass front (Gorilla Glass Victus 2), glass back (Gorilla Glass) or eco leather back, aluminum frame |
| [**SIM**](https://www.gsmarena.com/glossary.php3?term=sim) | Dual SIM (Nano-SIM, dual stand-by) |
|  | IP68 dust/water resistant (up to 1.5m for 30 min) |

|  |  |  |
| --- | --- | --- |
| **DISPLAY** | [**Type**](https://www.gsmarena.com/glossary.php3?term=display-type) | LTPO AMOLED, 1B colors, 120Hz, Dolby Vision, HDR10+, 1600 nits (typ), 2600 nits (HBM), 4500 nits (peak) |
| [**Size**](https://www.gsmarena.com/oppo_find_x7_ultra-12752.php) | 6.82 inches, 113.0 cm2 (~90.3% screen-to-body ratio) |
| [**Resolution**](https://www.gsmarena.com/glossary.php3?term=resolution) | 1440 x 3168 pixels (~510 ppi density) |
| [**Protection**](https://www.gsmarena.com/glossary.php3?term=screen-protection) | Corning Gorilla Glass Victus 2 |

|  |  |  |
| --- | --- | --- |
| **PLATFORM** | [**OS**](https://www.gsmarena.com/glossary.php3?term=os) | Android 14, ColorOS 14 |
| [**Chipset**](https://www.gsmarena.com/glossary.php3?term=chipset) | Qualcomm SM8650-AB Snapdragon 8 Gen 3 (4 nm) |
| [**CPU**](https://www.gsmarena.com/glossary.php3?term=cpu) | Octa-core (1x3.3 GHz Cortex-X4 & 5x3.2 GHz Cortex-A720 & 2x2.3 GHz Cortex-A520) |
| [**GPU**](https://www.gsmarena.com/glossary.php3?term=gpu) | Adreno 750 |

|  |  |  |
| --- | --- | --- |
| **MEMORY** | [**Card slot**](https://www.gsmarena.com/glossary.php3?term=memory-card-slot) | No |
| [**Internal**](https://www.gsmarena.com/glossary.php3?term=dynamic-memory) | 256GB 12GB RAM, 256GB 16GB RAM, 512GB 16GB RAM |
|  | UFS 4.0 |

|  |  |  |
| --- | --- | --- |
| **MAIN CAMERA** | [**Quad**](https://www.gsmarena.com/glossary.php3?term=camera) | 50 MP, f/1.8, 23mm (wide), 1.0"-type, 1.6µm, multi-directional PDAF, Laser AF, OIS 50 MP, f/2.6, 65mm (periscope telephoto), 1/1.56", 1.0µm, 2.8x optical zoom, multi-directional PDAF (25cm - ∞), OIS 50 MP, f/4.3, 135mm (periscope telephoto), 1/2.51", 6x optical zoom, Dual-Pixel PDAF (35cm - ∞), OIS 50 MP, f/2.0, 14mm, 123˚ (ultrawide), 1/1.95", 1.0µm, PDAF |
| [**Features**](https://www.gsmarena.com/glossary.php3?term=camera) | Hasselblad Color Calibration, LED flash, HDR, panorama |
| [**Video**](https://www.gsmarena.com/glossary.php3?term=camera) | 4K@30/60fps, 1080p@30/60/240fps; gyro-EIS; HDR, 10‑bit video, Dolby Vision |

|  |  |  |
| --- | --- | --- |
| **SELFIE CAMERA** | [**Single**](https://www.gsmarena.com/glossary.php3?term=secondary-camera) | 32 MP, f/2.4, 21mm (wide), 1/2.74", 0.8µm, PDAF |
| [**Features**](https://www.gsmarena.com/glossary.php3?term=secondary-camera) | Panorama |
| [**Video**](https://www.gsmarena.com/glossary.php3?term=secondary-camera) | 4K@30/60fps, 1080p@30fps, gyro-EIS |

|  |  |  |
| --- | --- | --- |
| **SOUND** | [**Loudspeaker**](https://www.gsmarena.com/glossary.php3?term=loudspeaker) | Yes, with stereo speakers |
| [**3.5mm jack**](https://www.gsmarena.com/glossary.php3?term=audio-jack) | No |

|  |  |  |
| --- | --- | --- |
| **COMMS** | [**WLAN**](https://www.gsmarena.com/glossary.php3?term=wi-fi) | Wi-Fi 802.11 a/b/g/n/ac/6e/7, dual-band, Wi-Fi Direct |
| [**Bluetooth**](https://www.gsmarena.com/glossary.php3?term=bluetooth) | 5.4, A2DP, LE, aptX HD, LHDC |
| [**Positioning**](https://www.gsmarena.com/glossary.php3?term=gnss) | GPS (L1+L5), BDS (B1I+B1c+B2a), GALILEO (E1+E5a), QZSS (L1+L5), GLONASS |
| [**NFC**](https://www.gsmarena.com/glossary.php3?term=nfc) | Yes; NFC-SIM, HCE, eSE, eID |
| [**Infrared port**](https://www.gsmarena.com/glossary.php3?term=irda) | Yes |
| [**Radio**](https://www.gsmarena.com/glossary.php3?term=fm-radio) | No |
| [**USB**](https://www.gsmarena.com/glossary.php3?term=usb) | USB Type-C 3.2, OTG |

|  |  |  |
| --- | --- | --- |
| **FEATURES** | [**Sensors**](https://www.gsmarena.com/glossary.php3?term=sensors) | Fingerprint (under display, optical), accelerometer, gyro, proximity, compass, color spectrum |
|  | Emergency SOS via satellite (messages and calls) |

|  |  |  |
| --- | --- | --- |
| **BATTERY** | [**Type**](https://www.gsmarena.com/glossary.php3?term=rechargeable-battery-types) | 5000 mAh, non-removable |
| [**Charging**](https://www.gsmarena.com/glossary.php3?term=battery-charging) | 100W wired, PD, 50% in 10 min, 100% in 26 min (advertised) 50W wireless 10W reverse wireless |

|  |  |  |
| --- | --- | --- |
| **MISC** | [**Colors**](https://www.gsmarena.com/glossary.php3?term=build) | Black, Dark Blue, Light Brown |
| [**Models**](https://www.gsmarena.com/glossary.php3?term=models) | PHY110 |